Navman Instructions (Updated 3 April 2006) 

 

These instructions are for Navman V3 and newer Software.

Platform and Software Supported 
iCN510 (V3 and newer) 
iCN520 (SmartST 2005 or newer) 
iCN530 (SmartST 2006 or newer) 
iCN550 (SmartST 2005 or newer) 
iCN620 (V3 and newer) 
iCN630 (V3 and newer) 
iCN635 (V3 and newer) 
iCN650 (V3 and newer) 
iCN7xx (SmartST 2006 or newer) 
Pocket PC (V3 and newer) 
PiN570

Platform and Software NOT Supported 
Pocket PC (V1) 
Pocket PC (V2) 
iCN510 (V2) 
iCN620 (V2) 
iCN630 (V1) 
iCN630 (V2) 
iCN3xx (SmartST 2005 and newer) 
If you are unsure which version you have, check in the ABOUT screen. 


Downloading the Pocket GPS Safety Camera Database 

1. Download from Pocket GPS Safety Camera Database page.

2. Login to PocketGPSWorld.Com and goto the Safety Camera Download page.

3. Select SatNav System NAVMAN, choose Continue then choose the database version you wish to use.

 

For this guide we are using the UK - Consolidated by Type option.

 

Extracting the Database on the PC

1. Extract the ZIP file contents to a directory on your PC, e.g. C:\temp 


Installing Pocket GPS Safety Camera Database 

 

1. Run Navman SmartST Desktop on your PC.

2. Connect your Navman Device. 

3. Click MAP | POI's to open the POI Editor.

4. Click FILE | OPEN and point to the folder where you extracted the ASC files , e.g. C:\Temp\POCKETGPS_UK_GATSO.ASC

5. You should now see the Speed Camera data in a screen below.

6. Click FILE | SAVE TO DEVICE
7. Now tick ACTIVE, VISUAL ALERT, IMPERIAL, 150, Increase the POI Visibility and also point to the BMP file you extracted earlier from the ZIP file, e.g. C:\Temp\pocketgps_uk_gatso.bmp

8. Now enter a name to appear within the Navman software

This should have now downloaded the data to your iCN or V3 software and you should now see it in there and be notified of the latest Speed Cameras