;;
;; Marvell SD8686 Windows XP Driver
;;
;;

[Version]
 DriverVer           = 01/05/2009,8.75.809.818
 Signature           = "$Chicago$"
 Compatible          = 1 
 Class               = Net
 ClassGUID           = {4d36e972-e325-11ce-bfc1-08002be10318} 
 Provider            = %MRVL% 
 CatalogFile = mrv86net.cat

[Manufacturer]
 %VER_VENDOR_NAME_STR% = DeviceList

[DeviceList]
 %SDIO_DESC_STR%     = MARVELL_SDIO1,        SD\VID_02df&PID_9103


;==========
[MARVELL_SDIO1.NT]
 AddReg    = MARVELL_SDIO1.reg, COMMON_SDIO.reg, COMMON_NDIS.reg.NT, COMMON.reg
 CopyFiles = MARVELL_DRIVER.copy.NT, MARVELL_APPLET.copy.NT
 BusType   = 1
 Characteristics= 0x84

[MARVELL_SDIO1.NT.Services]
 AddService= "SD8686", 2, MARVELL_DRIVER_SDIO.Service

[MARVELL_SDIO1.NT.CoInstallers]
 CopyFiles = MARVELL_COINSTALL.copy.NT
 AddReg    = MARVELL_COINSTALL.reg.NT

[MARVELL_SDIO1.reg]
 HKR,Ndi,DeviceID,0,"SDIO\VID_05A3&PID_8388"
 HKR,,VendorDesc,0,%SDIO_DESC_STR%


;###############################################################################

[MARVELL_COINSTALL.reg.NT]
;HKR,           ,CoInstallers32         ,0x00010000     ,"sd8686NDI.dll,NdiProc"

[MARVELL_DRIVER_SDIO.Service]
 DisplayName    = %MARVELL_SERVICE_DISPLAY_SDIO%
 ServiceType    = 1    ; SERVICE_KERNEL_DRIVER
 StartType      = 3    ; SERVICE_DEMAND_START
 ErrorControl   = 1    ; NORMAL
 ServiceBinary  = %12%\sd8686nd5.sys
 LoadOrderGroup = NDIS

[MARVELL_DRIVER.EventLog]
 AddReg         = MARVELL_DRIVER.EventLog.reg

[MARVELL_DRIVER.EventLog.reg]
 HKR,           ,EventMessageFile       ,0x00020000     ,"%%SystemRoot%%\System32\netevent.dll"
 HKR,           ,TypesSupported         ,0x00010001     ,7

[MARVELL_API.Register]
;dirid, subdir, filename, registration flags[, [optional timeout][, argument]]

;###############################################################################
;RegKey,SubKey          ,Name                   ,Type   ,Value
;-------------          -----                   -----   ------
[COMMON_SDIO.reg]
 HKR,NDI                ,Service                ,0      ,"sd8686"
 HKR,NDI                ,CardType               ,0      ,"SDIO"
 HKR,                   ,BusType                ,0      ,"0"
 HKR,                   ,DeviceVxDs             ,0      ,"sd8686nd5.sys"

[COMMON_NDIS.reg]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
;HKR,NDI                ,NdiInstaller           ,0      ,"sd8686NDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"sd8686"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.ME]
 HKR,                   ,RunningWin9X           ,0      ,"1"
 HKR,                   ,DevLoader              ,0      ,"*ndis"
 HKR,                   ,EnumPropPages          ,0      ,"netdi.dll,EnumPropPages"
;HKR,NDI                ,NdiInstaller           ,0      ,"sd8686NDI.dll,NdiProc"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"
 HKR,NDI\Interfaces     ,DefUpper               ,0      ,"ndis3"
 HKR,NDI\Interfaces     ,DefLower               ,0      ,"ethernet"
 HKR,NDIS               ,LogDriverName          ,0      ,"sd8686"
 HKR,NDIS               ,MajorNdisVersion       ,1      ,03
 HKR,NDIS               ,MinorNdisVersion       ,1      ,0a

[COMMON_NDIS.reg.NT]
;HKR,                   ,EnumPropPages32        ,0      ,"sd8686NDI.dll,NetPropPageProvider"
 HKR,NDI\Interfaces     ,UpperRange             ,0      ,"ndis5"
 HKR,NDI\Interfaces     ,LowerRange             ,0      ,"ethernet"

[COMMON.reg]
 HKR,                   ,MacIoctl               ,0      ,"1"
 HKR,                   ,SilentInstall          ,0      ,"1"
;Uncomment the line above to install without user interface prompts

;----------------------------------------------------------------------------
; RTS Threshold
;----------------------------------------------------------------------------
 HKR,defaults,RTSThresh,0,2347
; HKR,NDI\params\RTSThresh,,0,2346
 HKR,Ndi\params\RTSThresh,default,0,2347
 HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
 HKR,NDI\params\RTSThresh,type,0,int
;HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
 HKR,NDI\params\RTSThresh,min,0,0
 HKR,NDI\params\RTSThresh,max,0,2347
 HKR,NDI\params\RTSThresh,optional,0,1

;----------------------------------------------------------------------------
; Fragmentation Threshold
;----------------------------------------------------------------------------
 HKR,defaults,FragThresh,0,2346
; HKR,NDI\params\FragThresh,,0,2346
 HKR,Ndi\params\FragThresh,default,0,2346
 HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
 HKR,NDI\params\FragThresh,type,0,int
;HKR,NDI\params\FragThresh,flag,1,20,00,00,00
 HKR,NDI\params\FragThresh,min,0,256
 HKR,NDI\params\FragThresh,max,0,2346
 HKR,NDI\params\FragThresh,step,0,2
 HKR,NDI\params\FragThresh,optional,0,1
 
;----------------------------------------------------------------------------
; Adhoc mode 11g G Rate
;----------------------------------------------------------------------------
 HKR,defaults,AdhocGRate,       0,      4
; HKR,NDI\params\AdhocGRate,           ,       1,      4
 HKR,Ndi\params\AdhocGRate,Default,   0,      "0"
 HKR,NDI\params\AdhocGRate,ParamDesc, ,       %ADHOCGRATE_STR%
 HKR,NDI\params\AdhocGRate,type,      ,       enum
 HKR,NDI\params\AdhocGRate\enum,0,    ,       %ADHOCGRATE_NO%
 HKR,NDI\params\AdhocGRate\enum,1,    ,       %ADHOCGRATE_YES%
 HKR,NDI\params\AdhocGRate,optional,  0,      1

;----------------------------------------------------------------------------
; MAC address
;----------------------------------------------------------------------------
 HKR,defaults,MAC,0,4
 HKR,NDI\Params\MAC,ParamDesc  ,0  ,%MAC_ADDR_STR%
;HKR,NDI\Params\MAC,Flag       ,1  ,20,00,00,00
 HKR,NDI\Params\MAC,Type       ,0  ,edit
 HKR,NDI\Params\MAC,Default    ,0  ,%MAC_ADDR_DEFAULT%
 HKR,NDI\Params\MAC,LimitText  ,0  ,17
 HKR,NDI\Params\MAC,UpperCase  ,0  ,1
 HKR,NDI\Params\MAC,Optional   ,0  ,1


;----------------------------------------------------------------------------
; 802.11bg Channel Number
;----------------------------------------------------------------------------
 HKR,defaults,ChannelB,0,4
 HKR,NDI\Params\ChannelB,ParamDesc  ,0  ,%CHANNEL_B_STR%
 HKR,NDI\Params\ChannelB,Type       ,0  ,int
 HKR,NDI\Params\ChannelB,Default    ,0  ,1
 HKR,NDI\params\ChannelB,min        ,0  ,1
 HKR,NDI\params\ChannelB,max        ,0  ,11
 HKR,NDI\Params\ChannelB,Optional   ,0  ,1

;----------------------------------------------------------------------------
; Data Rate
;----------------------------------------------------------------------------
 HKR,defaults,DataRate          ,0      ,4
 HKR,NDI\Params\DataRate,ParamDesc  ,0  ,%DATA_RATE_STR%
 HKR,NDI\Params\DataRate,Type       ,0  ,enum
 HKR,NDI\Params\DataRate,Default    ,0  ,"3"
 HKR,NDI\params\DataRate,flag       ,1  ,20,00,00,00
 HKR,NDI\Params\DataRate,Optional   ,0  ,1
 HKR,NDI\params\DataRate\enum,0     ,0  , %DATARATE_1MBPS%
 HKR,NDI\params\DataRate\enum,1     ,0  ,%DATARATE_2MBPS%
 HKR,NDI\params\DataRate\enum,2     ,0  ,%DATARATE_5_5MBPS%
 HKR,NDI\params\DataRate\enum,3     ,0  ,%DATARATE_11MBPS%
 ;HKR,NDI\params\DataRate\enum,4     ,0  ,%DATARATE_22MBPS%
 HKR,NDI\params\DataRate\enum,5     ,0  ,%DATARATE_6MBPS%
 HKR,NDI\params\DataRate\enum,6     ,0  ,%DATARATE_9MBPS%
 HKR,NDI\params\DataRate\enum,7     ,0  ,%DATARATE_12MBPS%
 HKR,NDI\params\DataRate\enum,8     ,0  ,%DATARATE_18MBPS%
 HKR,NDI\params\DataRate\enum,9     ,0  ,%DATARATE_24MBPS%
 HKR,NDI\params\DataRate\enum,10    ,0  ,%DATARATE_36MBPS%
 HKR,NDI\params\DataRate\enum,11    ,0  ,%DATARATE_48MBPS%
 HKR,NDI\params\DataRate\enum,12    ,0  ,%DATARATE_54MBPS%
 ;HKR,NDI\params\DataRate\enum,13    ,0  ,%DATARATE_0MBPS%
 HKR,NDI\params\DataRate\enum,14    ,0  ,%DATARATE_AUTO%


;----------------------------------------------------------------------------
; Other Parameters available but not implemented in the INF
;----------------------------------------------------------------------------
;#define PARAM_NetworkMode                   "NetworkMode"
;#define PARAM_DesiredSSID                   "DesiredSSID"
;#define PARAM_Preamble                      "Preamble"
;#define PARAM_WepKey1                       "WepKey1"
;#define PARAM_WepKey2                       "WepKey2"
;#define PARAM_WepKey3                       "WepKey3"
;#define PARAM_WepKey4                       "WepKey4"
;#define PARAM_WepStatus                     "WepStatus"
;#define PARAM_TxWepKey                      "TxWepKey"
;#define PARAM_AuthMode                      "AuthMode"
;#define PARAM_TxPowerLevel                  "TxPower"
;#define PARAM_AuthenticationMode            "AuthenticationMode"
;#define PARAM_PrivacyFilter                 "PrivacyFilter"
;#define PARAM_BeaconPeriod                  "BeaconPeriod"
;#define PARAM_DtimPeriod                    "DtimPeriod"
;#define PARAM_AtimWindow                    "ATIMWindow"

;----------------------------------------------------------------------------
; WMM ACK Policy AC_VO
;----------------------------------------------------------------------------
 HKR,defaults,ACKPolicyAC_VO,             0,      4
 HKR,Ndi\params\ACKPolicyAC_VO,Default,   0,      "0"
 HKR,NDI\params\ACKPolicyAC_VO,ParamDesc, ,       %ACKPolicyAC_VO_STR%
 HKR,NDI\params\ACKPolicyAC_VO,type,      ,       enum
 HKR,NDI\Params\ACKPolicyAC_VO,Default    ,0      ,0
 HKR,NDI\params\ACKPolicyAC_VO\enum,0,    ,       %WMMACK%
 HKR,NDI\params\ACKPolicyAC_VO\enum,1,    ,       %WMM_NO_ACK%
 HKR,NDI\params\ACKPolicyAC_VO,optional,  0,      1

 ;----------------------------------------------------------------------------
; WMM ACK Policy AC_VI
;----------------------------------------------------------------------------
 HKR,defaults,ACKPolicyAC_VI,             0,      4
 HKR,Ndi\params\ACKPolicyAC_VI,Default,   0,      "0"
 HKR,NDI\params\ACKPolicyAC_VI,ParamDesc, ,       %ACKPolicyAC_VI_STR%
 HKR,NDI\params\ACKPolicyAC_VI,type,      ,       enum
 HKR,NDI\Params\ACKPolicyAC_VI,Default    ,0      ,0
 HKR,NDI\params\ACKPolicyAC_VI\enum,0,    ,       %WMMACK%
 HKR,NDI\params\ACKPolicyAC_VI\enum,1,    ,       %WMM_NO_ACK%
 HKR,NDI\params\ACKPolicyAC_VI,optional,  0,      1

 ;----------------------------------------------------------------------------
; WMM ACK Policy AC_BE
;----------------------------------------------------------------------------
 HKR,defaults,ACKPolicyAC_BE,             0,      4
 HKR,Ndi\params\ACKPolicyAC_BE,Default,   0,      "0"
 HKR,NDI\params\ACKPolicyAC_BE,ParamDesc, ,       %ACKPolicyAC_BE_STR%
 HKR,NDI\params\ACKPolicyAC_BE,type,      ,       enum
 HKR,NDI\Params\ACKPolicyAC_BE,Default    ,0      ,0
 HKR,NDI\params\ACKPolicyAC_BE\enum,0,    ,       %WMMACK%
 HKR,NDI\params\ACKPolicyAC_BE\enum,1,    ,       %WMM_NO_ACK%
 HKR,NDI\params\ACKPolicyAC_BE,optional,  0,      1

 ;----------------------------------------------------------------------------
; WMM ACK Policy AC_BK
;----------------------------------------------------------------------------
 HKR,defaults,ACKPolicyAC_BK,             0,      4
 HKR,Ndi\params\ACKPolicyAC_BK,Default,   0,      "0"
 HKR,NDI\params\ACKPolicyAC_BK,ParamDesc, ,       %ACKPolicyAC_BK_STR%
 HKR,NDI\params\ACKPolicyAC_BK,type,      ,       enum
 HKR,NDI\Params\ACKPolicyAC_BK,Default    ,0      ,0
 HKR,NDI\params\ACKPolicyAC_BK\enum,0,    ,       %WMMACK%
 HKR,NDI\params\ACKPolicyAC_BK\enum,1,    ,       %WMM_NO_ACK%
 HKR,NDI\params\ACKPolicyAC_BK,optional,  0,      1

;----------------------------------------------------------------------------
; Enable/Disable 802.11D
;----------------------------------------------------------------------------
 HKR,,EnableDot11d,             0,      0
 HKR,Ndi\params\EnableDot11d,Default,   0,      "0"
 HKR,NDI\params\EnableDot11d,ParamDesc, ,       %EnableDot11d%
 HKR,NDI\params\EnableDot11d,type,      ,       enum
 HKR,NDI\Params\EnableDot11d,Default,   0,      0
 HKR,NDI\params\EnableDot11d\enum,0,    ,       %DISABLE%
 HKR,NDI\params\EnableDot11d\enum,1,    ,       %ENABLE%
 HKR,NDI\params\EnableDot11d,optional,  0,      0

;----------------------------------------------------------------------------
; Enable/Disable 802.11H
;----------------------------------------------------------------------------
 HKR,,EnableDot11h,                     0,      "0"
 
;----------------------------------------------------------------------------
; Enable/Disable 802.11H DFSMode
;----------------------------------------------------------------------------
 HKR,,EnableDFSMode,                     0,      "0"

;----------------------------------------------------------------------------
; Sleep Period
;----------------------------------------------------------------------------
 HKR,defaults,SleepPeriod,0,4
 HKR,NDI\Params\SleepPeriod,ParamDesc  ,0  ,%SLEEP_PERIOD_STR%
 HKR,NDI\Params\SleepPeriod,Type       ,0  ,int
 HKR,NDI\Params\SleepPeriod,Default    ,0  ,10
 HKR,NDI\params\SleepPeriod,min        ,0  ,0
 HKR,NDI\params\SleepPeriod,max        ,0  ,60
 HKR,NDI\Params\SleepPeriod,Optional   ,0  ,10

;----------------------------------------------------------------------------
; Local Listen Interval
;----------------------------------------------------------------------------
 HKR,defaults,LocalListenInterval,0,4
 HKR,NDI\Params\LocalListenInterval,ParamDesc  ,0  ,%LOCAL_LISTEN_INTERVAL_STR%
 HKR,NDI\Params\LocalListenInterval,Type       ,0  ,int
 HKR,NDI\Params\LocalListenInterval,Default    ,0  ,0
 HKR,NDI\params\LocalListenInterval,min        ,0  ,0
 HKR,NDI\params\LocalListenInterval,max        ,0  ,20
 HKR,NDI\Params\LocalListenInterval,Optional   ,0  ,1

;----------------------------------------------------------------------------
; Inactivity Timeout
;----------------------------------------------------------------------------
 HKR,defaults,InactivityTimeout,0,4
 HKR,NDI\Params\InactivityTimeout,ParamDesc  ,0  ,%INACTIVITY_TIMEOUT_STR%
 HKR,NDI\Params\InactivityTimeout,Type       ,0  ,int
 HKR,NDI\Params\InactivityTimeout,Default    ,0  ,50
 HKR,NDI\params\InactivityTimeout,min        ,0  ,1
 HKR,NDI\params\InactivityTimeout,max        ,0  ,1000
 HKR,NDI\Params\InactivityTimeout,Optional   ,0  ,1
 
;----------------------------------------------------------------------------
; ATIM Window
;----------------------------------------------------------------------------
 HKR,defaults,AtimWindow,0,4
 HKR,NDI\Params\AtimWindow,ParamDesc  ,0  ,%ATIM_WINDOW_STR%
 HKR,NDI\Params\AtimWindow,Type       ,0  ,int
 HKR,NDI\Params\AtimWindow,Default    ,0  ,0
 HKR,NDI\params\AtimWindow,min        ,0  ,0
 HKR,NDI\params\AtimWindow,max        ,0  ,50
 HKR,NDI\Params\AtimWindow,Optional   ,0  ,1 
 
;----------------------------------------------------------------------------
; Power Save Mode
;----------------------------------------------------------------------------
 HKR,defaults,PowerSaveMode,0,0
; HKR,NDI\params\PowerSaveMode,,0,0
 HKR,Ndi\params\PowerSaveMode,default,0,"0"
 HKR,NDI\params\PowerSaveMode,ParamDesc,,%POWER_SAVE_MODE_STR%
 HKR,NDI\params\PowerSaveMode,type,,enum
 HKR,NDI\params\PowerSaveMode,flag,1,30,00,00,00
 HKR,NDI\params\PowerSaveMode\enum,0,,%DISABLE%
 HKR,NDI\params\PowerSaveMode\enum,1,,%IEEE_PS%
 ;HKR,NDI\params\PowerSaveMode\enum,2,,%UAPSD%
 ;HKR,NDI\params\PowerSaveMode\enum,3,,%MRVL_INACTIVITY_TIMEOUT%
 ;HKR,NDI\params\PowerSaveMode\enum,4,,%MRVL_PROP_PS%
 ;HKR,NDI\params\PowerSaveMode\enum,5,, %IEE_PS_PLUS_HOST_SLEEP%
 HKR,NDI\params\PowerSaveMode,optional,0,1
 
;----------------------------------------------------------------------------
; BEACON PERIOD
;----------------------------------------------------------------------------
 HKR,defaults,BeaconPeriod,0,4
 HKR,NDI\Params\BeaconPeriod,ParamDesc  ,0  ,%BEACON_PERIOD_STR%
 HKR,NDI\Params\BeaconPeriod,Type       ,0  ,int
 HKR,NDI\Params\BeaconPeriod,Default    ,0  ,100
 HKR,NDI\params\BeaconPeriod,min        ,0  ,10
 HKR,NDI\params\BeaconPeriod,max        ,0  ,1000
 HKR,NDI\Params\BeaconPeriod,Optional   ,0  ,1 

;----------------------------------------------------------------------------
; RADIO OFF
;----------------------------------------------------------------------------
 HKR,,RadioOff,                     0,      "0"
 HKR,Ndi\params\RadioOff,Default,   0,      "0"
 HKR,NDI\params\RadioOff,ParamDesc, ,       %RADIO_OFF_STR%
 HKR,NDI\params\RadioOff,type,      ,       enum
 HKR,NDI\Params\RadioOff,Default,   0,      0
 HKR,NDI\params\RadioOff\enum,0,    ,       %ENABLE_RADIO%
 HKR,NDI\params\RadioOff\enum,1,    ,       %DISABLE_RADIO%
 HKR,NDI\params\RadioOff,optional,  0,      1

;----------------------------------------------------------------------------
; Region Code
;----------------------------------------------------------------------------
 HKR,defaults,RegionCode,           0,       1
 HKR,Ndi\params\RegionCode,Default,   0,      "0"
 HKR,NDI\params\RegionCode,ParamDesc, ,       %RegionCode%
 HKR,NDI\params\RegionCode,type,      ,       enum
 HKR,NDI\Params\RegionCode,Default,   0,      0
 HKR,NDI\params\RegionCode\enum,0,    ,       %DEFAULT%
 HKR,NDI\params\RegionCode\enum,1,    ,       %USA%
 HKR,NDI\params\RegionCode\enum,2,    ,       %EUROPE%
 HKR,NDI\params\RegionCode\enum,3,    ,       %SPAIN%
 HKR,NDI\params\RegionCode\enum,4,    ,       %FRANCE%
 HKR,NDI\params\RegionCode\enum,5,    ,       %JAPAN%
 HKR,NDI\params\RegionCode,optional,  0,      0
;----------------------------------------------------------------------------

;----------------------------------------------------------------------------
; Rx, Tx Antenna
;----------------------------------------------------------------------------
 HKR,Antenna,         Tx,                0x00010001, 1 ; Tx Antenna 0 = Diversity, 1 = Antenna 1, 2 = Antenna 2
 HKR,Antenna,         Rx,                0x00010001, 1 ; Rx Antenna 0 = Diversity, 1 = Antenna 1, 2 = Antenna 2

;###############################################################################
[DestinationDirs]
;CopyFiles Section      = Destination Directory ID -- see layout.inf
;-----------------        ------------------------
 DefaultDestDir         = 11 ; Win9x=%windir%\system Win2k=%windir%\system32
 MARVELL_DRIVER.copy      = 11
 MARVELL_DRIVER.copy.ME   = 11
 MARVELL_DRIVER.copy.NT   = 12 ; Win2k=%windir%\system32\drivers

[MARVELL_NDI.copy]
;sd8686NDI.dll

[MARVELL_NDI.copy.ME]
;sd8686NDI.dll

[MARVELL_COINSTALL.copy.NT]
;sd8686NDI.dll

[MARVELL_DRIVER.copy]
 sd8686nd5.sys
;MacIoctl.vxd

[MARVELL_DRIVER.copy.ME]
 sd8686nd5.sys
;MacIoctl.vxd

[MARVELL_DRIVER.copy.NT]
 sd8686nd5.sys

[MARVELL_APPLET.copy]

[MARVELL_APPLET.copy.ME]

[MARVELL_APPLET.copy.NT]

[SourceDisksNames]
;Source Disk ID         = Disk Name
;--------------           ---------
 1                      = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]      ; Win9x
;File Name              = Source Disk ID
;---------                --------------
 sd8686nd5.sys             = 1
;MacIoctl.vxd           = 1,win9x
;sd8686NDI.dll          = 1,win9x

[SourceDisksFiles.ME]   ; WinMe
 sd8686nd5.sys             = 1
;MacIoctl.vxd           = 1,win9x
;sd8686NDI.dll          = 1,win9x

[SourceDisksFiles.X86]  ; Win2k/Xp
 sd8686nd5.sys             = 1
;sd8686nd5.sys             = 1,winxp
;sd8686NDI.dll          = 1,win2k

;###############################################################################
[Strings]
;String ID              = String Text
;---------                -----------
 MRVL                   = "Marvell Semiconductor, Inc."
 VER_VENDOR_STR         = "Marvell"
 VER_VENDOR_NAME_STR    = "Marvell Semiconductor, Inc."

; MARVELL_SERVICE_DISPLAY_SDIO  = "Marvell SD8686 Wireless LAN SDIO Driver"
 MARVELL_SERVICE_DISPLAY_SDIO  = "SD8686"
 INSTALL_DISK_STR       = "Wireless Networking Install Disk"

 RTSTHRESH_STR          = "RTS Threshold"
 FRAGTHRESH_STR         = "Fragmentation Threshold"
 POWER_SAVE_MODE_STR    = "Power Save Mode"
 BAND_STR               = "Band to Use"
 MAC_ADDR_STR           = "Factory MAC Address Fallback"
 MAC_ADDR_DEFAULT       = "00-01-02-03-04-05"
 DATA_RATE_STR          = "Transmit Data Rate"
 CHANNEL_B_STR          = "802.11bg Ad Hoc Channel Number"
 TX_ANTENNA_STR         = "Transmit Antenna"
 RX_ANTENNA_STR         = "Receive Antenna"
 SCAN_DWELL_STR         = "Scan Channel Dwell Time"
 SCAN_DWELL_ASSOC_STR   = "Scan Channel Dwell Time when Associated"
 SDIO_DESC_STR          = "Marvell sd8686 Wireless LAN SDIO Adapter"
 ACKPolicyAC_BK_STR     = "WMM AC_BK ACK Policy"
 ACKPolicyAC_BE_STR     = "WMM AC_BE ACK Policy"
 ACKPolicyAC_VI_STR     = "WMM AC_VI ACK Policy"
 ACKPolicyAC_VO_STR     = "WMM AC_VO ACK Policy"
 EnableDot11d           = "802.11D Support"
 ADHOCGRATE_STR         = "Use G Rate For Ad Hoc"
 SLEEP_PERIOD_STR       = "Sleep Period"
 LOCAL_LISTEN_INTERVAL_STR = "Local Listen Interval"
 INACTIVITY_TIMEOUT_STR = "Inactivity Timeout" 
 ATIM_WINDOW_STR = "ATIM Window" 
 BEACON_PERIOD_STR = "Beacon Period" 
 RADIO_OFF_STR = "Radio Off"
 ADHOCGRATE_NO = "no"
 ADHOCGRATE_YES = "yes"
 DATARATE_1MBPS = "1 Mbps"
 DATARATE_2MBPS = "2 Mbps"
 DATARATE_5_5MBPS = "5.5 Mbps"
 DATARATE_11MBPS = "11 Mbps"
 DATARATE_22MBPS = "22 Mbps"
 DATARATE_6MBPS = "6 Mbps"
 DATARATE_9MBPS = "9 Mbps"
 DATARATE_12MBPS = "12 Mbps"
 DATARATE_18MBPS = "18 Mbps"
 DATARATE_24MBPS = "24 Mbps"
 DATARATE_36MBPS = "36 Mbps"
 DATARATE_48MBPS = "48 Mbps"
 DATARATE_54MBPS = "54 Mbps"
 DATARATE_0MBPS = "0 Mbps"
 DATARATE_AUTO = "Auto"
 WMMACK = "ACK"
 WMM_NO_ACK = "No Ack"
 ENABLE = "Enable"
 DISABLE = "Disable"
 IEEE_PS = "IEEE 802.11 Power Save"
 UAPSD = "UAPSD"
 MRVL_INACTIVITY_TIMEOUT = "Marvell Inactivity Timeout"
 MRVL_PROP_PS = "Marvell Proprietary PS"
 IEE_PS_PLUS_HOST_SLEEP = "(EXP)IEEE PS + HostSleep"
 ENABLE_RADIO = "Enable Radio"
 DISABLE_RADIO = "Disable Radio"
 RegionCode = "Region Code"
 DEFAULT = "Default"
 USA = "USA"
 EUROPE = "Europe"
 SPAIN = "Spain"
 FRANCE = "France"
 JAPAN = "Japan"