What Does This Do?
This utility installs the PEGA-WL100\WL110 Driver Update to add the following enhancements:
Displays the MAC address in the "Wireless LAN Detailed Settings" window.
Adds compatibility for more Wireless Access Points.
Applicable Products and Operating Systems (see full list...)
Model:PEG-NX70VOperating System:
Palm OS? Software 5.x

IMPORTANT: This file is only for use with the models identified. Not all models are sold in all countries.
Important Notes
This update application requires that you have approximately 300KB of available memory in your CLI¨¦ handheld. Before installing this application, follow these steps to confirm that there is enough memory available.
Tap the "Home" icon.
Tap the "Menu" icon and select "App".
Tap "Info..." from the App drop-down list. All internal data information is displayed.
Tap "Size" at the bottom of the screen.
Check the "Free Space:..." listed.
Tap the "Done" button to exit.
During the installation of this update, be sure that you are logged in as the Administrator or as a user with Administrative rights.
Make sure that Palm? Desktop for CLI¨¦ software is installed on your PC from the installation CD-ROM supplied with your CLI¨¦ handheld and that the PC is configured to be able to perform a HotSync? operation.
To ensure that no other program interferes with the installation, save all work and close all other programs. The Taskbar should be clear of applications before proceeding.
It is highly recommended to print out these instructions as a reference during the installation process.

Download and Installation Instructions
Download the WL100_ENUS.PRC file to a temporary or download directory (please note this directory for reference).
WARNING!!: Please perform a soft reset on your CLI¨¦ ? handheld BEFORE performing the update installation by pressing the small reset button on the left side of your CLI¨¦? handheld. For more detailed information, refer to the CLI¨¦ ? Read This First manual.
On your PC, start the Palm? Desktop for CLI¨¦? software.
Click the Install icon. The Install tool wizard starts.
At the "Install Tool" window, select the appropriate user name from the user list.
Click "Add."
Navigate to the location to which you saved the update file.
Select the application file "WL100_ENUS.PRC" and click "Open."
Click "Done."
Place your CLI¨¦ ? handheld on the cradle, and perform a HotSync? operation.
After the HotSync operation finishes, you are prompted to reset your CLI¨¦ ? handheld.
Tap "Reset."
NOTE: When installing the WL100_ENUS.PRC update file from a Memory Stick? media, it is necessary to perform a soft reset of the CLI¨¦? handheld after the installation.
Confirm a Successful Installation
Tap the "Home" icon on the CLI¨¦? handheld.
Tap the "Menu" icon, and select "App".
Tap "Info" from the App drop-down list. All internal data information is displayed.
Tap "Version" at the bottom of the screen. The software version for each item is displayed.
Scroll down the list and confirm that the CF WL100inf file is version 1.20.
Tap the "Done" button to exit.
NOTE: If the version number is not 1.20, re-download the WL100_ENUS.PRC and install it again.
Contact Information
If you have difficulty installing the update, contact the Sony Customer Information Center: 1-877-760-SONY (7669). 

Additional Information
Please read following conditions carefully.
Please follow the instructions when operating this program.
Palm, Palm OS and HotSync are trademarks of Palm, Inc. and (or) its subsidiaries.
CLI¨¦, Memory Stick and Sony are trademarks of Sony Corporation.
Copyright 2003 Sony Electronics, Inc.